#!/usr/bin/env bash
#
# Build tests for STM32F103RE BigTreeTech (SKR E3 DIP v1.0)
#

# exit on first failure
set -e

#
# Build with the default configurations
#
restore_configs
opt_set MOTHERBOARD BOARD_BTT_SKR_E3_DIP
opt_set SERIAL_PORT 1
opt_set SERIAL_PORT_2 -1
exec_test $1 $2 "BigTreeTech SKR E3 DIP v1.0 - Basic Configuration" "$3"

restore_configs
opt_set MOTHERBOARD BOARD_BTT_SKR_CR6
opt_set SERIAL_PORT -1
opt_set SERIAL_PORT_2 2
opt_set TEMP_SENSOR_BED 1
opt_enable CR10_STOCKDISPLAY \
           NOZZLE_AS_PROBE Z_MIN_PROBE_USES_Z_MIN_ENDSTOP_PIN Z_SAFE_HOMING \
           PROBE_ACTIVATION_SWITCH PROBE_TARE PROBE_TARE_ONLY_WHILE_INACTIVE \
           PROBING_HEATERS_OFF PREHEAT_BEFORE_PROBING
opt_disable NOZZLE_TO_PROBE_OFFSET
exec_test $1 $2 "BigTreeTech SKR CR6 PROBE_ACTIVATION_SWITCH, Probe Tare" "$3"

# clean up
restore_configs
