Filetype: IR library file
Version: 1
#
# Model: Yamaha RAV15 and NoName Unknown Audio remote
name: Play
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 44 00 00 00
#
# Model: Western Digital Unknown
name: Power
type: parsed
protocol: NECext
address: 84 79 00 00
command: 12 ED 00 00
#
name: Play
type: parsed
protocol: NECext
address: 84 79 00 00
command: 0A F5 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 84 79 00 00
command: 05 FA 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 84 79 00 00
command: 00 FF 00 00
#
name: Next
type: parsed
protocol: NECext
address: 84 79 00 00
command: 01 FE 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 84 79 00 00
command: 02 FD 00 00
#
# Model: Yamaha RX-V375
name: Power
type: parsed
protocol: NEC
address: 7E 00 00 00
command: 2A 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1A 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1C 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1B 00 00 00
#
# Model: SVEN HT-415
name: Power
type: parsed
protocol: NEC
address: 41 00 00 00
command: 42 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 41 00 00 00
command: 0B 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 41 00 00 00
command: 1B 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 41 00 00 00
command: 56 00 00 00
#
# Model: HUAYU AKB74475490
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: B0 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: BA 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8F 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8E 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
#
# Model: Samsung HW-K450 Soundbar
#
name: Power
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4637 4376 612 419 584 420 584 420 583 421 582 1427 531 1477 531 472 532 472 557 1452 556 1451 557 1451 557 1452 556 447 557 448 556 449 555 449 555 4453 554 450 554 450 554 451 553 450 554 451 553 451 553 451 553 450 554 1455 553 1454 554 1454 554 451 553 1454 554 1454 554 1455 553 1454 554 451 553 450 554 450 554 1455 553 55439 4554 4458 555 449 555 449 555 450 554 450 554 1455 553 1454 554 451 553 450 554 1454 554 1454 554 1454 554 1455 553 450 554 451 553 451 553 451 553 4453 554 451 553 451 552 451 553 451 553 451 553 451 553 451 553 451 553 1455 553 1455 553 1455 553 451 553 1455 553 1455 553 1455 553 1455 553 451 553 451 552 451 553 1455 553
#
name: Play
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4636 4380 612 392 612 394 610 394 610 419 583 1399 557 1452 556 473 556 448 556 1428 581 1453 555 1453 555 1453 555 449 555 450 554 451 553 452 552 4457 551 452 552 452 552 452 552 452 552 452 552 1457 551 452 552 1457 551 452 552 452 552 453 551 1457 552 1457 551 452 552 1457 551 452 552 1457 551 1457 551 1457 552 452 552 55450 4551 4461 553 451 553 452 552 452 552 452 552 1456 552 1456 552 452 552 452 552 1456 552 1456 552 1456 552 1456 552 452 552 452 552 453 551 453 551 4456 551 453 551 453 551 453 551 453 551 453 551 1457 551 453 551 1457 552 453 551 454 550 454 550 1457 552 1457 551 454 550 1457 551 454 550 1458 551 1457 551 1458 550 454 550
#
name: Vol_up
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4640 4405 583 420 583 421 582 421 583 422 581 1427 531 1478 530 473 531 472 557 1452 557 1452 556 1452 556 1452 556 448 556 448 556 449 555 450 554 4454 554 451 553 451 553 451 553 451 553 1455 554 1455 553 1455 553 451 553 1455 553 1456 553 1456 553 451 553 451 553 451 553 451 554 1455 554 451 553 452 553 451 553 1456 553 55447 4556 4458 555 449 555 450 554 450 554 450 554 1455 553 1455 553 451 553 451 553 1455 553 1455 553 1455 553 1455 553 451 553 451 553 451 553 451 553 4454 553 451 553 450 554 451 553 450 554 1455 553 1455 553 1455 553 451 553 1455 553 1455 553 1455 553 451 553 451 553 451 553 450 554 1455 553 451 553 451 553 451 553 1455 553
#
name: Vol_dn
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4636 4378 613 393 611 392 612 393 611 393 557 1451 558 1450 610 420 583 421 557 1427 581 1452 556 1452 556 1452 556 448 555 449 555 450 554 450 554 4455 553 451 553 451 553 451 553 451 553 451 553 451 553 452 552 1456 553 1456 552 1456 553 1456 552 451 553 1456 553 1456 552 1456 553 451 553 451 553 452 552 451 553 1456 552 55452 4553 4461 553 450 554 451 553 451 553 451 553 1456 553 1456 552 451 553 451 553 1456 552 1455 553 1455 553 1455 553 451 553 451 553 451 553 451 553 4456 552 451 553 451 553 451 553 451 553 451 553 451 553 451 553 1456 552 1455 553 1455 553 1455 553 451 553 1455 553 1456 552 1456 552 451 553 451 553 451 553 451 553 1456 552
#
name: Prev
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 255 113623 4638 4378 613 391 612 392 559 446 558 446 558 1477 531 1477 532 472 532 472 532 1476 532 1476 532 1476 532 1477 531 473 555 449 555 449 555 450 554 4455 554 450 554 450 554 450 554 450 554 1455 554 1455 554 450 554 1455 554 450 555 450 554 450 554 1455 554 451 553 451 553 1455 554 450 554 1455 554 1456 553 1455 554 450 554
#
name: Next
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4557 4430 611 392 610 394 559 445 559 446 558 1451 558 1477 531 448 556 472 532 1476 532 1477 532 1477 531 1477 531 473 556 449 555 449 555 450 554 4454 554 450 554 450 554 450 554 450 555 450 554 450 554 1455 554 1455 554 450 554 450 554 450 554 1455 554 1455 554 1455 553 451 553 450 554 1455 554 1455 554 1455 554 450 554 55458 4555 4459 554 450 554 450 554 450 554 450 554 1455 553 1455 553 450 554 450 554 1455 553 1455 553 1455 553 1455 553 450 554 450 554 450 554 450 554 4454 554 450 554 450 554 450 554 451 553 450 554 450 554 1455 553 1455 553 451 553 450 554 450 554 1455 553 1455 553 1455 553 450 554 451 553 1455 554 1455 553 1455 553 450 554
#
name: Mute
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 4639 4406 586 418 585 393 559 447 557 447 557 1477 532 1477 532 472 532 472 532 1476 533 1476 532 1476 532 1476 532 473 555 449 555 449 555 449 555 4455 554 450 554 450 554 450 554 450 554 1455 554 450 554 450 554 450 554 1455 554 1455 553 1455 553 450 554 450 554 1455 554 1455 554 1455 554 450 554 450 554 450 554 1455 554 55454 4557 4458 555 449 555 449 555 450 554 450 554 1455 554 1455 553 450 554 450 554 1455 554 1455 554 1454 554 1455 554 450 554 450 554 450 555 450 554 4455 553 450 554 450 554 450 554 450 554 1455 554 450 554 450 554 450 554 1455 554 1455 554 1455 553 450 554 450 554 1455 554 1455 553 1455 554 450 554 450 554 450 554 1455 554
#
# Model: Edifier R1850DB
name: Power
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 46 B9 00 00
#
name: Play
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 5E A1 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 05 FA 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 49 B6 00 00
#
name: Next
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 02 FD 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 1E E1 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 41 BE 00 00
#
# Model: Grundig CMS 5000
name: Power
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 10 EF 00 00
# Also Pause
name: Play
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 02 FD 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0D F2 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 17 E8 00 00
#
name: Next
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 13 EC 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 11 EE 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0C F3 00 00
#
# Model: Panasonic SA-PM193
name: Power
type: parsed
protocol: Kaseikyo
address: AC 02 20 00
command: D1 03 00 00
# CD play/pause, tape play also exists but probably less commonly used
name: Play
type: parsed
protocol: Kaseikyo
address: AA 02 20 00
command: A0 00 00 00
# same as above
name: Pause
type: parsed
protocol: Kaseikyo
address: AA 02 20 00
command: A0 00 00 00
#
name: Vol_up
type: parsed
protocol: Kaseikyo
address: A0 02 20 00
command: 00 02 00 00
#
name: Vol_dn
type: parsed
protocol: Kaseikyo
address: A0 02 20 00
command: 10 02 00 00
#
name: Next
type: parsed
protocol: Kaseikyo
address: AC 02 20 01
command: A1 00 00 00
#
name: Prev
type: parsed
protocol: Kaseikyo
address: AC 02 20 01
command: 91 00 00 00
#
name: Mute
type: parsed
protocol: Kaseikyo
address: A0 02 20 00
command: 20 03 00 00
#
# Model: NAD C316BEE
name: Power
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 25 DA 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 94 6B 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 88 77 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 8C 73 00 00
#
name: Play
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 01 FE 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 4A B5 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 05 FA 00 00
#
name: Next
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 06 F9 00 00
#
# Model: Dutch Originals Sound Bar
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 00 00 00 00
command: 6A 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 6A 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 5E 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 85 00 00 00
#
# Sony audio remote RM-SC3
name: Power
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 15 00 00 00
#
name: Vol_up
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 13 00 00 00
#
name: Play
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 32 00 00 00
#
name: Pause
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 39 00 00 00
#
# Model: Sony MHC_GSX75
#
name: Pause
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 38 00 00 00
#
# Model: Elac EA101EQ-G
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 46 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 18 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 55 00 00 00
#
# Model: Philips FW750C
#
name: Vol_up
type: parsed
protocol: RC5
address: 10 00 00 00
command: 10 00 00 00
#
name: Vol_dn
type: parsed
protocol: RC5
address: 10 00 00 00
command: 11 00 00 00
#
name: Play
type: parsed
protocol: RC5
address: 14 00 00 00
command: 35 00 00 00
#
name: Pause
type: parsed
protocol: RC5
address: 14 00 00 00
command: 36 00 00 00
#
name: Mute
type: parsed
protocol: RC5
address: 10 00 00 00
command: 0D 00 00 00
#
name: Power
type: parsed
protocol: RC5
address: 14 00 00 00
command: 0C 00 00 00
#
# Model: Pioneer VSX-D1-S
#
name: Vol_up
type: parsed
protocol: NECext
address: 00 7F 00 00
command: 0A F5 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 00 7F 00 00
command: 5C A3 00 00
#
name: Power
type: parsed
protocol: NECext
address: 00 7F 00 00
command: 1E E1 00 00
# # Model: Adastra WA215
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 44 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 49 00 00 00
#
# Model: Adcom GTP500II
#
name: Power
type: parsed
protocol: NEC42
address: 51 00 00 00
command: 00 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC42
address: 51 00 00 00
command: 1F 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC42
address: 51 00 00 00
command: 1E 00 00 00
#
# Model: Aiwa RC-T506
#
name: Power
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 00 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 4D 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 4E 00 00 00
#
# Model: AIWA XR-EM300
#
name: Mute
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 4C 00 00 00
#
# Model: ASR EMITTER1HD
#
name: Power
type: parsed
protocol: RC5
address: 10 00 00 00
command: 0C 00 00 00
#
# Model: Auna AV2_CD508
#
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4B 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 04 00 00 00
command: 04 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5E 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
#
# Model: CambridgeAudio 650A
#
name: Next
type: parsed
protocol: RC5
address: 14 00 00 00
command: 2B 00 00 00
#
name: Pause
type: parsed
protocol: RC5
address: 14 00 00 00
command: 30 00 00 00
#
# Model: AEG
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 02 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 01 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0A 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0E 00 00 00
#
# Model: AIWA NSXR71
#
name: Play
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 40 00 00 00
#
name: Pause
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 44 00 00 00
#
name: Pause
type: parsed
protocol: NEC42
address: 6E 00 00 00
command: 41 00 00 00
#
# Model: Denon RC_1199
#
name: Power
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 03 00 00 00
#
name: Vol_up
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 04 00 00 00
#
name: Vol_dn
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 05 00 00 00
#
name: Mute
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 06 00 00 00
#
name: Prev
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 47 00 00 00
#
name: Next
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 46 00 00 00
#
name: Prev
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 0F 00 00 00
#
name: Next
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 0E 00 00 00
#
name: Pause
type: parsed
protocol: Kaseikyo
address: 51 54 32 01
command: 3F 00 00 00
#
# Model: Fisher SLIM-1500
#
name: Power
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 06 00 00 00
#
name: Pause
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 13 00 00 00
#
name: Play
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 13 00 00 00
#
name: Pause
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 1B 00 00 00
#
name: Mute
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: A0 00 00 00
#
name: Vol_up
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 20 00 00 00
#
name: Vol_dn
type: parsed
protocol: Samsung32
address: A2 00 00 00
command: 60 00 00 00
#
# Model: GPX cd_radio
#
name: Pause
type: parsed
protocol: Samsung32
address: 81 00 00 00
command: 09 00 00 00
#
name: Next
type: parsed
protocol: Samsung32
address: 81 00 00 00
command: 11 00 00 00
#
# Model: GPX HC221B
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 04 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 02 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 00 00 00 00
command: 00 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 01 00 00 00
#
# Model: LG
#
name: Power
type: parsed
protocol: Samsung32
address: 10 00 00 00
command: 1E 00 00 00
#
name: Mute
type: parsed
protocol: Samsung32
address: 10 00 00 00
command: 1F 00 00 00
#
name: Pause
type: parsed
protocol: Samsung32
address: 10 00 00 00
command: 05 00 00 00
#
# Model: Marantz RC2100DR_CD
#
name: Prev
type: parsed
protocol: RC5
address: 14 00 00 00
command: 21 00 00 00
#
name: Next
type: parsed
protocol: RC5
address: 14 00 00 00
command: 20 00 00 00
#
name: Next
type: parsed
protocol: RC5
address: 14 00 00 00
command: 34 00 00 00
#
# Model: Marantz RC2100DR_CDR
#
name: Power
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 0C 00 00 00
#
name: Prev
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 21 00 00 00
#
name: Next
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 20 00 00 00
#
name: Next
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 34 00 00 00
#
name: Pause
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 30 00 00 00
#
name: Pause
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 36 00 00 00
#
name: Play
type: parsed
protocol: RC5
address: 1A 00 00 00
command: 35 00 00 00
#
# Model: Onkyo DX-7333
#
name: Pause
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 1F E0 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 1C E3 00 00
#
name: Play
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 1B E4 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 01 FE 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 00 FF 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 1E E1 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 2C 00 00
command: 1D E2 00 00
#
# Model: Panasonic SC-HC58
#
name: Pause
type: parsed
protocol: Kaseikyo
address: AC 02 20 00
command: 01 00 00 00
#
# Model: Philips CD_720
#
name: Vol_dn
type: parsed
protocol: RC5
address: 14 00 00 00
command: 11 00 00 00
#
name: Vol_up
type: parsed
protocol: RC5
address: 14 00 00 00
command: 10 00 00 00
#
# Model: Philips CD_Player_723
#
name: Prev
type: parsed
protocol: RC5
address: 14 00 00 00
command: 32 00 00 00
#
# Model: Rockola juke
#
name: Power
type: parsed
protocol: NEC
address: 4D 00 00 00
command: 00 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 4D 00 00 00
command: 0F 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 4D 00 00 00
command: 10 00 00 00
#
# Model: Sony CFD-S35CP
#
name: Vol_up
type: parsed
protocol: SIRC15
address: 44 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC15
address: 44 00 00 00
command: 13 00 00 00
#
name: Play
type: parsed
protocol: SIRC15
address: 64 00 00 00
command: 32 00 00 00
#
name: Pause
type: parsed
protocol: SIRC15
address: 64 00 00 00
command: 39 00 00 00
#
name: Pause
type: parsed
protocol: SIRC15
address: 64 00 00 00
command: 38 00 00 00
#
name: Prev
type: parsed
protocol: SIRC15
address: 64 00 00 00
command: 3A 00 00 00
#
name: Next
type: parsed
protocol: SIRC15
address: 64 00 00 00
command: 3B 00 00 00
#
# Model: SONY minidisk-deck
#
name: Power
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 15 00 00 00
#
name: Play
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 2A 00 00 00
#
name: Pause
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 29 00 00 00
#
name: Pause
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 28 00 00 00
#
name: Prev
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 20 00 00 00
#
name: Prev
type: parsed
protocol: SIRC
address: 0F 00 00 00
command: 2B 00 00 00
#
# Model: Sony RM-R52_RCD-W500C_Deck-A
#
name: Play
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 32 00 00 00
#
name: Pause
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 39 00 00 00
#
name: Pause
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 38 00 00 00
#
name: Prev
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 30 00 00 00
#
name: Next
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 31 00 00 00
#
name: Next
type: parsed
protocol: SIRC
address: 11 00 00 00
command: 34 00 00 00
#
# Model: Sony RM-R52_RCD-W500C_Deck-B
#
name: Play
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 2A 00 00 00
#
name: Pause
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 29 00 00 00
#
name: Pause
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 28 00 00 00
#
name: Prev
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 20 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 21 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 5A 19 00 00
command: 2C 00 00 00
#
# Model: TEAC RC-505_Remote_Control_Unit
#
name: Play
type: parsed
protocol: NECext
address: 86 61 00 00
command: 08 F7 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 86 61 00 00
command: 05 FA 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 86 61 00 00
command: 09 F6 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 86 61 00 00
command: 0D F2 00 00
#
name: Next
type: parsed
protocol: NECext
address: 86 61 00 00
command: 0C F3 00 00
#
# Model: Unkown KC-806
#
name: Power
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 1C E3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 00 FF 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 04 FB 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 17 E8 00 00
#
name: Next
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 02 FD 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 01 FE 00 00
#
# Model: Winnes KC809
#
name: Pause
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 16 E9 00 00
#
# Model: Denon RC1253
#
name: Power
type: parsed
protocol: Kaseikyo
address: 41 54 32 00
command: 05 00 00 00
#
name: Vol_up
type: parsed
protocol: Kaseikyo
address: 41 54 32 00
command: 70 01 00 00
#
name: Vol_dn
type: parsed
protocol: Kaseikyo
address: 41 54 32 00
command: 71 01 00 00
#
name: Mute
type: parsed
protocol: Kaseikyo
address: 41 54 32 00
command: 72 01 00 00
#
name: Prev
type: parsed
protocol: Kaseikyo
address: 41 54 32 00
command: 22 00 00 00
#
# Model: Douk ST-01_Pro
#
name: Power
type: parsed
protocol: NECext
address: AA 33 00 00
command: 45 FF 00 00
#
name: Play
type: parsed
protocol: NECext
address: AA 33 00 00
command: 44 FF 00 00
#
name: Prev
type: parsed
protocol: NECext
address: AA 33 00 00
command: 40 FF 00 00
#
name: Next
type: parsed
protocol: NECext
address: AA 33 00 00
command: 43 FF 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: AA 33 00 00
command: 09 FF 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: AA 33 00 00
command: 15 FF 00 00
#
name: Mute
type: parsed
protocol: NECext
address: AA 33 00 00
command: 47 FF 00 00
#
# Model: Edifier r1280t
#
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 3C C3 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 4D B2 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 2B D4 00 00
#
# Model: Edifier r1700bt
#
name: Power
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 01 FE 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 09 F6 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 0C F3 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 00 FF 00 00
#
# Model: Edifier r1855db
#
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 06 F9 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 47 B8 00 00
#
# Model: Edifier r2000db
#
name: Power
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 00 FF 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 01 FE 00 00
#
# Model: Emotiva PT100_TA100
#
name: Power
type: parsed
protocol: NECext
address: 00 79 00 00
command: 80 7F 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 00 79 00 00
command: 99 66 00 00
#
# Model: Grundig CMS_5000
#
name: Pause
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 05 FA 00 00
#
# Model: Harman Kardon AVI200
#
name: Power
type: parsed
protocol: NECext
address: 80 70 00 00
command: C0 3F 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 80 70 00 00
command: C1 3E 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 80 70 00 00
command: C7 38 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 80 70 00 00
command: C8 37 00 00
#
# Model: DTR-7
#
name: Power
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 04 FB 00 00
#
name: Power
type: parsed
protocol: NECext
address: D2 6C 00 00
command: 47 B8 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 02 FD 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 03 FC 00 00
#
name: Mute
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 05 FA 00 00
#
# Model: Logitech Z906
#
name: Power
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 80 7F 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 02 A0 00 00
command: EA 15 00 00
#
# Model: NAD712
#
name: Power
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 80 7F 00 00
#
# Model: NAD Amp_1
#
name: Power
type: parsed
protocol: NECext
address: 87 7C 00 00
command: C8 37 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 02 FD 00 00
#
# Model: Onkyo
#
name: Power
type: parsed
protocol: NECext
address: D2 6C 00 00
command: CB 34 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 6C 00 00
command: 54 AB 00 00
#
# Model: Onkyo RC627S
#
name: Power
type: parsed
protocol: NECext
address: D2 03 00 00
command: 04 FB 00 00
#
name: Power
type: parsed
protocol: NECext
address: D2 04 00 00
command: 47 B8 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: D2 03 00 00
command: 02 FD 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: D2 03 00 00
command: 03 FC 00 00
#
name: Play
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1B E4 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1F E0 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1C E3 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 03 00 00
command: 8B 74 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 03 00 00
command: 8A 75 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1E E1 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1D E2 00 00
#
# Model: Onkyo RC866M_Receiver
#
name: Prev
type: parsed
protocol: NECext
address: D2 02 00 00
command: 90 6F 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 02 00 00
command: 80 7F 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 02 00 00
command: 8F 70 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 02 00 00
command: 91 6E 00 00
#
name: Play
type: parsed
protocol: NECext
address: D2 02 00 00
command: 8D 72 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 02 00 00
command: 8E 71 00 00
#
# Model: Onkyo RC898M
#
name: Mute
type: parsed
protocol: NECext
address: D2 11 00 00
command: 05 FA 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: D2 19 00 00
command: 82 7D 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: D2 19 00 00
command: 83 7C 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 14 00 00
command: 90 6F 00 00
#
name: Prev
type: parsed
protocol: NECext
address: D2 14 00 00
command: 81 7E 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 14 00 00
command: 80 7F 00 00
#
name: Next
type: parsed
protocol: NECext
address: D2 14 00 00
command: 8F 70 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 14 00 00
command: 91 6E 00 00
#
name: Play
type: parsed
protocol: NECext
address: D2 14 00 00
command: 8D 72 00 00
#
name: Pause
type: parsed
protocol: NECext
address: D2 14 00 00
command: 8E 71 00 00
#
# Model: Panasonic N2QAYB000210
#
name: Pause
type: parsed
protocol: Kaseikyo
address: A2 02 20 00
command: 02 00 00 00
#
name: Pause
type: parsed
protocol: Kaseikyo
address: A2 02 20 00
command: 62 00 00 00
#
name: Play
type: parsed
protocol: Kaseikyo
address: A2 02 20 00
command: A2 00 00 00
#
name: Play
type: parsed
protocol: Kaseikyo
address: AC 02 20 02
command: B1 02 00 00
#
# Model: Panasonic SA_PM602
#
name: Play
type: parsed
protocol: Kaseikyo
address: AC 02 20 00
command: 61 00 00 00
#
# Model: Panasonic SC-PMX92-94
#
name: Next
type: parsed
protocol: Kaseikyo
address: AC 02 20 00
command: 31 00 00 00
#
name: Prev
type: parsed
protocol: Kaseikyo
address: AC 02 20 00
command: 21 00 00 00
#
# Model: Philips BTD2180
#
name: Power
type: parsed
protocol: RC6
address: 04 00 00 00
command: 0C 00 00 00
#
name: Vol_up
type: parsed
protocol: RC6
address: 04 00 00 00
command: 10 00 00 00
#
name: Mute
type: parsed
protocol: RC6
address: 04 00 00 00
command: 2C 00 00 00
#
name: Vol_dn
type: parsed
protocol: RC6
address: 04 00 00 00
command: 11 00 00 00
#
name: Prev
type: parsed
protocol: RC6
address: 04 00 00 00
command: 21 00 00 00
#
name: Pause
type: parsed
protocol: RC6
address: 04 00 00 00
command: 31 00 00 00
#
name: Next
type: parsed
protocol: RC6
address: 04 00 00 00
command: 20 00 00 00
#
name: Prev
type: parsed
protocol: RC6
address: 04 00 00 00
command: 83 00 00 00
#
# Model: Pioneer AXD7741
#
name: Power
type: parsed
protocol: Pioneer
address: A5 00 00 00
command: 1C 00 00 00
#
name: Vol_up
type: parsed
protocol: Pioneer
address: A5 00 00 00
command: 0A 00 00 00
#
name: Vol_dn
type: parsed
protocol: Pioneer
address: A5 00 00 00
command: 0B 00 00 00
#
# Model: Pioneer VSX-D1-S
#
name: Vol_dn
type: parsed
protocol: NECext
address: 00 7F 00 00
command: 06 F9 00 00
#
# Model: Pioneer XXD3105
#
name: Play
type: parsed
protocol: Pioneer
address: AA 00 00 00
command: 0C 00 00 00
#
name: Pause
type: parsed
protocol: Pioneer
address: AA 00 00 00
command: 5B 00 00 00
#
# Model: Portta Toslink_Audio_Switcher
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 17 00 00 00
#
# Model: Pyle P2203ABTU
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1C 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0F 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 05 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0B 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4D 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 54 00 00 00
#
# Model: Rega IO
#
name: Prev
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 08 00 00 00
#
# Model: Revo Superconnect_BZAWDFB0315H2
#
name: Power
type: parsed
protocol: NEC
address: 40 00 00 00
command: 02 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 40 00 00 00
command: 01 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 40 00 00 00
command: 12 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 40 00 00 00
command: 59 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 40 00 00 00
command: 18 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 40 00 00 00
command: 58 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 40 00 00 00
command: 5B 00 00 00
#
# Model: Rio Sonic_Blue_059PXC
#
name: Power
type: parsed
protocol: NECext
address: 82 13 00 00
command: 84 7B 00 00
#
name: Play
type: parsed
protocol: NECext
address: 82 13 00 00
command: 85 7A 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 82 13 00 00
command: 90 6F 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 82 13 00 00
command: 83 7C 00 00
#
name: Next
type: parsed
protocol: NECext
address: 82 13 00 00
command: 87 78 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 82 13 00 00
command: 80 7F 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 82 13 00 00
command: 8A 75 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 82 13 00 00
command: 81 7E 00 00
#
# Model: SiriusXM Onyx_EZR
#
name: Power
type: parsed
protocol: RC5X
address: 1B 00 00 00
command: 0C 00 00 00
#
name: Mute
type: parsed
protocol: RC5X
address: 1B 00 00 00
command: 0D 00 00 00
#
# Model: SMSL RC-8A
#
name: Power
type: parsed
protocol: NECext
address: 12 34 00 00
command: 01 FE 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 12 34 00 00
command: 0A F5 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 12 34 00 00
command: 0B F4 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 12 34 00 00
command: 09 F6 00 00
#
# Model: SMSL RC-8C
#
name: Power
type: parsed
protocol: NECext
address: 12 36 00 00
command: 01 FE 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 12 36 00 00
command: 0A F5 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 12 36 00 00
command: 0B F4 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 12 36 00 00
command: 09 F6 00 00
#
# Model: Sony Amp
#
name: Power
type: parsed
protocol: SIRC15
address: 30 00 00 00
command: 15 00 00 00
#
name: Vol_up
type: parsed
protocol: SIRC15
address: 30 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC15
address: 30 00 00 00
command: 13 00 00 00
#
name: Mute
type: parsed
protocol: SIRC15
address: 30 00 00 00
command: 14 00 00 00
#
# Model: Sony I-WXH-80
#
name: Power
type: parsed
protocol: NEC
address: 01 00 00 00
command: 02 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 01 00 00 00
command: 01 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 01 00 00 00
command: 0B 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 01 00 00 00
command: 06 00 00 00
#
# Model: Sony MHC-GS300AV
#
name: Power
type: parsed
protocol: SIRC15
address: 10 00 00 00
command: 15 00 00 00
#
name: Vol_up
type: parsed
protocol: SIRC15
address: 10 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC15
address: 10 00 00 00
command: 13 00 00 00
#
# Model: Sony RMT-AA320U_AV
#
name: Pause
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 38 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 31 00 00 00
#
name: Prev
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 30 00 00 00
#
name: Prev
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 7D 00 00 00
#
# Model: Sony RM_AMU009_Sony_Audio_System_CMT
#
name: Prev
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 30 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 31 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 34 00 00 00
#
# Model: Sony STR-DH590
#
name: Prev
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 33 00 00 00
#
name: Next
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 34 00 00 00
#
# Model: Firetv EVG487
#
name: Power
type: parsed
protocol: NEC
address: 01 00 00 00
command: 67 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 01 00 00 00
command: 38 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 01 00 00 00
command: 3C 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 01 00 00 00
command: 3D 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 01 00 00 00
command: 8C 00 00 00
#
# Model: Audac IMEO2
#
name: Power
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1C E3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 21 DE 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2B D4 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1D E2 00 00
#
name: Play
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 13 EC 00 00
#
name: Next
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 14 EB 00 00
#
# Model: Bestisan7020
#
name: Power
type: parsed
protocol: NECext
address: 29 A1 00 00
command: 7F 80 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 29 A1 00 00
command: 9B 64 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 29 A1 00 00
command: 9E 61 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 29 A1 00 00
command: 9F 60 00 00
#
# Model: Bose CINEMATE_1_SR
#
name: Power
type: parsed
protocol: NECext
address: BA A0 00 00
command: 4C B3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: BA A0 00 00
command: 03 FC 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: BA A0 00 00
command: 02 FD 00 00
#
name: Mute
type: parsed
protocol: NECext
address: BA A0 00 00
command: 01 FE 00 00
#
# Model: Bose Solo_5
#
name: Next
type: parsed
protocol: NECext
address: BA A0 00 00
command: 5A A5 00 00
#
name: Prev
type: parsed
protocol: NECext
address: BA A0 00 00
command: 59 A6 00 00
#
name: Pause
type: parsed
protocol: NECext
address: BA A0 00 00
command: 56 A9 00 00
#
name: Pause
type: parsed
protocol: NECext
address: BA A0 00 00
command: 1A E5 00 00
#
# Model: Bose Solo_Soundbar
#
name: Mute
type: parsed
protocol: NECext
address: BA A0 00 00
command: 01 FD 00 00
#
# Model: Bose Soundbar_300
#
name: Power
type: parsed
protocol: NECext
address: BA 4B 00 00
command: 4C B3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: BA 4B 00 00
command: 03 FC 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: BA 4B 00 00
command: 02 FD 00 00
#
name: Mute
type: parsed
protocol: NECext
address: BA 4B 00 00
command: 01 FE 00 00
#
name: Prev
type: parsed
protocol: NECext
address: BA 4B 00 00
command: 57 A8 00 00
#
# Model: Amz snd_bar
#
name: Power
type: parsed
protocol: NEC
address: 35 00 00 00
command: 09 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 35 00 00 00
command: 45 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 35 00 00 00
command: 1B 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 35 00 00 00
command: 51 00 00 00
#
# Model: Soundblasterx
#
name: Power
type: parsed
protocol: NECext
address: 83 22 00 00
command: 08 F7 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 83 22 00 00
command: 0C F3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 83 22 00 00
command: 0A F5 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 83 22 00 00
command: 01 FE 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 83 22 00 00
command: 07 F8 00 00
#
name: Next
type: parsed
protocol: NECext
address: 83 22 00 00
command: 06 F9 00 00
#
# Model: Canton Smart10
#
name: Mute
type: parsed
protocol: NECext
address: 00 FB 00 00
command: 1E E1 00 00
#
name: Power
type: parsed
protocol: NECext
address: 00 FB 00 00
command: 1D E2 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 00 FB 00 00
command: 18 E7 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 00 FB 00 00
command: 0A F5 00 00
#
name: Next
type: parsed
protocol: NECext
address: 00 FB 00 00
command: 0D F2 00 00
#
# Model: YARRA 3DX
#
name: Power
type: parsed
protocol: NECext
address: 0A 1D 00 00
command: 01 FE 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 0A 1D 00 00
command: 03 FC 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 0A 1D 00 00
command: 08 F7 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 0A 1D 00 00
command: 0A F5 00 00
#
# Model: Craig CHT912
#
name: Power
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0C 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 02 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 05 00 00 00
#
# Model: Craig CHT921
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 12 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 03 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 01 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1E 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1F 00 00 00
#
# Model: Craig CHT939
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1F 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
#
# Model: Soundbar creative_stage
#
name: Power
type: parsed
protocol: NEC
address: 20 00 00 00
command: 09 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 06 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 07 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1E 00 00 00
#
# Model: Denon RC-1230
#
name: Power
type: parsed
protocol: Kaseikyo
address: 52 54 32 00
command: 83 00 00 00
#
name: Mute
type: parsed
protocol: Kaseikyo
address: 52 54 32 00
command: 86 00 00 00
#
name: Vol_up
type: parsed
protocol: Kaseikyo
address: 52 54 32 00
command: 84 00 00 00
#
name: Vol_dn
type: parsed
protocol: Kaseikyo
address: 52 54 32 00
command: 85 00 00 00
#
# Model: Hisense HS215
#
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 20 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: 34 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: 34 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 21 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 22 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 04 00 00 00
command: 23 00 00 00
#
# Model: Hitachi HSB40B16
#
name: Power
type: parsed
protocol: NEC
address: 5B 00 00 00
command: 80 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 5B 00 00 00
command: 88 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 5B 00 00 00
command: 82 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 5B 00 00 00
command: 83 00 00 00
#
# Model: iLive ITP280B_Remote
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0C 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1E 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 42 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 41 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
#
# Model: iLive Soundbar
#
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 14 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 10 00 00 00
#
# Model: JBL 5_1_Soundbar
#
name: Power
type: parsed
protocol: NECext
address: 84 74 00 00
command: FF 00 00 00
#
# Model: JBL CINEMA_SB120
#
name: Power
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 53 AC 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 02 BD 00 00
command: AD 52 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 26 D9 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 28 D7 00 00
#
name: Next
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 27 D8 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 25 DA 00 00
#
# Model: JVC THBY370A
#
name: Power
type: parsed
protocol: NEC
address: 01 00 00 00
command: 00 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 01 00 00 00
command: 08 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 01 00 00 00
command: 09 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 01 00 00 00
command: 01 00 00 00
#
# Model: Klipsch Soundbar
#
name: Power
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1E 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 80 00 00 00
command: 01 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 80 00 00 00
command: 03 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 80 00 00 00
command: 06 00 00 00
#
# Model: Larksound L200
#
name: Vol_up
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 19 E6 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 16 E9 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 09 F6 00 00
#
name: Next
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 5E A1 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 0C F3 00 00
#
name: Play
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 18 E7 00 00
#
name: Power
type: parsed
protocol: NECext
address: 30 0F 00 00
command: 45 BA 00 00
#
# Model: LG SJ4
#
name: Power
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 1E 00 00 00
#
name: Vol_up
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 17 00 00 00
#
name: Vol_dn
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 16 00 00 00
#
name: Mute
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 1F 00 00 00
#
name: Play
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 4F 00 00 00
#
name: Prev
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 06 00 00 00
#
# Model: LG AKB74815321
#
name: Next
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 07 00 00 00
#
# Model: LG NB5541
#
name: Pause
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 4F 00 00 00
#
name: Pause
type: parsed
protocol: Samsung32
address: 2C 00 00 00
command: 05 00 00 00
#
# Model: Majority K2_SoundBar
#
name: Power
type: parsed
protocol: NEC
address: 20 00 00 00
command: 41 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 42 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 43 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1A 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 20 00 00 00
command: 4F 00 00 00
#
# Model: Onn sound_bar_and_subwoofer
#
name: Vol_up
type: parsed
protocol: NECext
address: 83 22 00 00
command: 16 E9 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 83 22 00 00
command: 0F F0 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 83 22 00 00
command: 15 EA 00 00
#
name: Power
type: parsed
protocol: NECext
address: 83 22 00 00
command: 0C F3 00 00
#
# Model: Panasonic SCH-TB8
#
name: Power
type: parsed
protocol: Kaseikyo
address: A0 02 20 00
command: D0 03 00 00
#
# Model: Pheanoo P27
#
name: Power
type: parsed
protocol: NECext
address: 83 B6 00 00
command: 4D B2 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 83 B6 00 00
command: 43 BC 00 00
#
# Model: Philips HTL2161B_Soundbar
#
name: Power
type: parsed
protocol: RC6
address: 10 00 00 00
command: 0C 00 00 00
#
name: Vol_up
type: parsed
protocol: RC6
address: 10 00 00 00
command: 10 00 00 00
#
name: Vol_dn
type: parsed
protocol: RC6
address: 10 00 00 00
command: 11 00 00 00
#
# Model: Philips HTL2163_Soundbar
#
name: Mute
type: parsed
protocol: RC6
address: 10 00 00 00
command: 0D 00 00 00
#
# Model: Philips TAB5105_79
#
name: Power
type: parsed
protocol: RC6
address: 10 00 00 00
command: C7 00 00 00
#
name: Next
type: parsed
protocol: RC6
address: 10 00 00 00
command: 20 00 00 00
#
name: Prev
type: parsed
protocol: RC6
address: 10 00 00 00
command: 21 00 00 00
#
name: Play
type: parsed
protocol: RC6
address: 10 00 00 00
command: 2C 00 00 00
#
# Model: Polk RE9114_1
#
name: Power
type: parsed
protocol: NECext
address: C8 91 00 00
command: 00 FF 00 00
#
name: Mute
type: parsed
protocol: NECext
address: C8 91 00 00
command: 20 DF 00 00
#
name: Prev
type: parsed
protocol: NECext
address: C8 91 00 00
command: 26 D9 00 00
#
name: Pause
type: parsed
protocol: NECext
address: C8 91 00 00
command: 21 DE 00 00
#
name: Next
type: parsed
protocol: NECext
address: C8 91 00 00
command: 24 DB 00 00
#
# Model: POLK RE9641_1
#
name: Vol_up
type: parsed
protocol: NECext
address: C8 91 00 00
command: 1E E1 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: C8 91 00 00
command: 1F E0 00 00
#
# Model: Promethean ActivSoundBar_ASB-40
#
name: Power
type: parsed
protocol: NEC
address: 80 00 00 00
command: 05 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 80 00 00 00
command: 02 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 80 00 00 00
command: 08 00 00 00
#
# Model: Quantis LSW-1
#
name: Power
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 12 ED 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 1D E2 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 1A E5 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 03 FC 00 00
#
# Model: RCA RTS7110B2
#
name: Power
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 5C 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 45 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 45 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 4E 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 55 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 8A 00 00 00
command: 59 00 00 00
#
# Model: Sennheiser Ambeo_Soundbar
#
name: Power
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0B 00 00 00
#
name: Vol_up
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0D 00 00 00
#
name: Vol_dn
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0E 00 00 00
#
name: Mute
type: parsed
protocol: RC5
address: 13 00 00 00
command: 0C 00 00 00
#
# Model: Sonos ARC_Beam_Playbar_Playbase
#
name: Vol_up
type: parsed
protocol: NECext
address: 80 D9 00 00
command: 8A 75 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 80 D9 00 00
command: 88 77 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 80 D9 00 00
command: 8C 73 00 00
#
# Model: Sony Old_XBR
#
name: Power
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 15 00 00 00
#
name: Vol_up
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 13 00 00 00
#
name: Mute
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 14 00 00 00
#
# Model: Sony Soundbar_HT-XT3
#
name: Play
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 32 00 00 00
#
name: Pause
type: parsed
protocol: SIRC20
address: 10 01 00 00
command: 39 00 00 00
#
# Model: TaoTronics TT-SK023_Sound_Bar
#
name: Power
type: parsed
protocol: NEC
address: 80 00 00 00
command: 12 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 80 00 00 00
command: 0D 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1E 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 80 00 00 00
command: 0A 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1F 00 00 00
#
# Model: Taotronics TT-SK026
#
name: Power
type: parsed
protocol: NECext
address: D9 14 00 00
command: 6D 92 00 00
#
name: Mute
type: parsed
protocol: NECext
address: D9 14 00 00
command: 6E 91 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: D9 14 00 00
command: 4F B0 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: D9 14 00 00
command: 50 AF 00 00
#
# Model: TCL TS5010
#
name: Pause
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
#
# Model: Teufel Cinebase_Soundbar
#
name: Power
type: parsed
protocol: NECext
address: EF 01 00 00
command: 25 DA 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: EF 01 00 00
command: 14 EB 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: EF 01 00 00
command: 13 EC 00 00
#
name: Mute
type: parsed
protocol: NECext
address: EF 01 00 00
command: 28 D7 00 00
#
# Model: Toshiba SBX4250
#
name: Power
type: parsed
protocol: NECext
address: 45 BD 00 00
command: 12 ED 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 45 BD 00 00
command: 1F E0 00 00
#
name: Play
type: parsed
protocol: NECext
address: 45 BD 00 00
command: 1F E0 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 45 BD 00 00
command: BD 42 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 45 BD 00 00
command: 60 9F 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 45 BD 00 00
command: 61 9E 00 00
#
# Model: Vizio SB3651_E6
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 41 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 48 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 8B 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 8A 00 00 00
#
# Model: Vizio V51-H6
#
name: Play
type: parsed
protocol: NEC
address: 00 00 00 00
command: 8E 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 8E 00 00 00
#
# Model: Binnifa Live1T
#
name: Mute
type: parsed
protocol: NEC
address: 20 00 00 00
command: 50 00 00 00
#
# Model: Yamaha BAR400
#
name: Power
type: parsed
protocol: NEC
address: 78 00 00 00
command: CC 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 78 00 00 00
command: 1E 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 78 00 00 00
command: 1F 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 78 00 00 00
command: 9C 00 00 00
#
# Model: Audioengine a5
#
name: Mute
type: parsed
protocol: NECext
address: 00 FD 00 00
command: 03 FC 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 00 FD 00 00
command: 09 F6 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 00 FD 00 00
command: 07 F8 00 00
#
# Model: Biseoamz DY29S
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1C 00 00 00
#
# Model: Bumpboxx
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 46 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
#
# Model: Como audio
#
name: Power
type: parsed
protocol: NEC
address: 77 00 00 00
command: F1 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 77 00 00 00
command: F3 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 77 00 00 00
command: F7 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 77 00 00 00
command: FB 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 77 00 00 00
command: FC 00 00 00
#
# Model: Craig CHT729
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0C 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 47 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
#
# Model: Craig CHT904
#
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0E 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1A 00 00 00
#
# Model: Creative z5400
#
name: Power
type: parsed
protocol: NEC
address: 08 00 00 00
command: 10 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 08 00 00 00
command: 1A 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 08 00 00 00
command: 0E 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 08 00 00 00
command: 16 00 00 00
#
# Model: DollarTec BT5AmpBoard
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
#
# Model: EASTERN DA_9000
#
name: Power
type: parsed
protocol: NEC
address: A0 00 00 00
command: 1D 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: A0 00 00 00
command: 18 00 00 00
#
# Model: Edifier AirPulse_A80
#
name: Power
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 00 FF 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 19 E6 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 1C E3 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 18 E7 00 00
#
# Model: Edifier R1280DB
#
name: Prev
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 06 F9 00 00
#
name: Next
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 08 F7 00 00
#
# Model: Edifier R1700BT
#
name: Vol_up
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 2B D4 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 3C C3 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 1A E5 00 00
#
# Model: Edifier R1700BTs
#
name: Prev
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 44 BB 00 00
#
# Model: Edifier R2800
#
name: Mute
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 09 F6 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 01 FE 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 02 FD 00 00
#
# Model: Edifier RC80B
#
name: Next
type: parsed
protocol: NECext
address: 10 E7 00 00
command: 5D A2 00 00
#
# Model: Edifier S360DB
#
name: Power
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 1C E3 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 0C F3 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 0F F0 00 00
#
name: Next
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 03 FC 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 78 0E 00 00
command: 40 BF 00 00
#
# Model: Fluance AI40
#
name: Power
type: parsed
protocol: NECext
address: 3F 5C 00 00
command: 18 E7 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 3F 5C 00 00
command: 55 AA 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 3F 5C 00 00
command: 59 A6 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 3F 5C 00 00
command: 15 EA 00 00
#
name: Next
type: parsed
protocol: NECext
address: 3F 5C 00 00
command: 16 E9 00 00
#
# Model: Dream Aurora_AC6923
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 57 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 03 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 10 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 13 00 00 00
#
# Model: Quacker LED_Speaker
#
name: Prev
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0D F2 00 00
#
# Model: Geneva Sound_System_Model_L
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 00 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 06 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0C 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0B 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0D 00 00 00
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
#
# Model: IBIZA PORT_15_UHF
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 48 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1D 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
#
# Model: JBL Cinema_CB150
#
name: Power
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1B E4 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 14 EB 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 13 EC 00 00
#
# Model: JBL LSR4326P
#
name: Vol_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 14 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 08 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 00 00 00 00
command: 00 00 00 00
#
# Model: JBL On_Stage_IIIP_Speaker
#
name: Mute
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 19 E6 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 12 ED 00 00
#
name: Next
type: parsed
protocol: NECext
address: 40 AF 00 00
command: 05 FA 00 00
#
# Model: JVC D62BM
#
name: Play
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0D F2 00 00
#
# Model: KEF LSX_Speakers
#
name: Power
type: parsed
protocol: NEC
address: 80 00 00 00
command: 02 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 80 00 00 00
command: 04 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 80 00 00 00
command: 4B 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 80 00 00 00
command: 4A 00 00 00
#
# Model: Klipsch fives
#
name: Power
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1A 00 00 00
#
# Model: Klipsch r15pm
#
name: Power
type: parsed
protocol: NEC
address: 02 00 00 00
command: 0A 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 02 00 00 00
command: 0D 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 02 00 00 00
command: 1C 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 02 00 00 00
command: 07 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 02 00 00 00
command: 02 00 00 00
#
# Model: Logi WD216XM
#
name: Power
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 02 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 08 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 00 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 01 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 05 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 04 00 00 00
#
# Model: Z906
#
name: Vol_up
type: parsed
protocol: NECext
address: 02 A0 00 00
command: AA 55 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 6A 95 00 00
#
# Model: Microlab RC071
#
name: Vol_up
type: parsed
protocol: NEC
address: 01 00 00 00
command: 11 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 01 00 00 00
command: 10 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: 01 00 00 00
command: 02 00 00 00
#
# Model: Microlab SOLO11
#
name: Prev
type: parsed
protocol: NEC
address: 01 00 00 00
command: 5A 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 01 00 00 00
command: 5B 00 00 00
#
# Model: Naim Muso
#
name: Power
type: parsed
protocol: RC5
address: 15 00 00 00
command: 0C 00 00 00
#
name: Mute
type: parsed
protocol: RC5
address: 15 00 00 00
command: 0D 00 00 00
#
name: Vol_up
type: parsed
protocol: RC5
address: 15 00 00 00
command: 10 00 00 00
#
name: Vol_dn
type: parsed
protocol: RC5
address: 15 00 00 00
command: 11 00 00 00
#
name: Next
type: parsed
protocol: RC5
address: 15 00 00 00
command: 20 00 00 00
#
# Model: Sangean RC30
#
name: Vol_up
type: parsed
protocol: NEC42
address: 01 00 00 00
command: 0C 00 00 00
#
# Model: Sony Amp_STR-DE875
#
name: Power
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 2E 00 00 00
#
name: Power
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 2F 00 00 00
#
name: Play
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 0C 00 00 00
#
name: Pause
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 0C 00 00 00
#
# Model: Sony SRS-GU10iP
#
name: Power
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 15 00 00 00
#
name: Mute
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 14 00 00 00
#
name: Play
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 28 00 00 00
#
name: Vol_up
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 12 00 00 00
#
name: Vol_dn
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 13 00 00 00
#
name: Next
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 29 00 00 00
#
name: Prev
type: parsed
protocol: SIRC15
address: 99 00 00 00
command: 2A 00 00 00
#
# Model: Steljes Desktop_Speakers
#
name: Power
type: parsed
protocol: NECext
address: 85 23 00 00
command: 99 66 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 85 23 00 00
command: 57 A8 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 85 23 00 00
command: 47 B8 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 85 23 00 00
command: 97 68 00 00
#
# Model: Teufel 3SIXTY
#
name: Power
type: parsed
protocol: NEC
address: FD 00 00 00
command: E2 00 00 00
#
name: Mute
type: parsed
protocol: NEC
address: FD 00 00 00
command: E1 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: FD 00 00 00
command: E7 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: FD 00 00 00
command: B9 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: FD 00 00 00
command: EA 00 00 00
#
# Model: Teufel CEM500RC
#
name: Mute
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1C 00 00 00
#
name: Vol_up
type: parsed
protocol: NEC
address: 80 00 00 00
command: 13 00 00 00
#
name: Vol_dn
type: parsed
protocol: NEC
address: 80 00 00 00
command: 17 00 00 00
#
# Model: Toshiba RM-V329
#
name: Power
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 12 ED 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 11 EE 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 10 EF 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 13 EC 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 03 FC 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 07 F8 00 00
#
name: Next
type: parsed
protocol: NECext
address: 2D D3 00 00
command: 06 F9 00 00
#
# Model: Technics EUR646496
#
name: Power
type: parsed
protocol: Kaseikyo
address: 80 02 20 00
command: D0 03 00 00
#
name: Play
type: parsed
protocol: Kaseikyo
address: 90 02 20 00
command: A0 00 00 00
#
name: Next
type: parsed
protocol: Kaseikyo
address: AA 02 20 01
command: A0 00 00 00
#
name: Pause
type: parsed
protocol: Kaseikyo
address: AA 02 20 00
command: 00 00 00 00
#
# Model: terratec m3po
#
name: Mute
type: parsed
protocol: RC5X
address: 0A 00 00 00
command: 2F 00 00 00
#
name: Play
type: parsed
protocol: RC5X
address: 0A 00 00 00
command: 31 00 00 00
#
name: Pause
type: parsed
protocol: RC5X
address: 0A 00 00 00
command: 0F 00 00 00
#
name: Pause
type: parsed
protocol: RC5X
address: 0A 00 00 00
command: 2C 00 00 00
#
# Model: X4 TECH_TU-1200
#
name: Power
type: parsed
protocol: NEC
address: 00 00 00 00
command: 04 00 00 00
#
# Model: YAMAHA AX-380
#
name: Power
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1F 00 00 00
#
# Model: Yamaha RAS5
#
name: Power
type: parsed
protocol: NECext
address: 7E 81 00 00
command: 2A D4 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1A E4 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1B E5 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1C E2 00 00
#
# Model: Yamaha RAV203_V473170_US
#
name: Mute
type: parsed
protocol: RC5
address: 00 00 00 00
command: 0D 00 00 00
#
name: Pause
type: parsed
protocol: RC5
address: 05 00 00 00
command: 29 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 59 00 00 00
#
name: Play
type: parsed
protocol: RC5
address: 05 00 00 00
command: 35 00 00 00
#
# Model: Yamaha WS19340
#
name: Power
type: parsed
protocol: NEC
address: 78 00 00 00
command: 0F 00 00 00
#
name: Play
type: parsed
protocol: NEC
address: 78 00 00 00
command: 02 00 00 00
#
name: Prev
type: parsed
protocol: NEC
address: 78 00 00 00
command: 04 00 00 00
#
name: Next
type: parsed
protocol: NEC
address: 78 00 00 00
command: 03 00 00 00
#
name: Pause
type: parsed
protocol: NEC
address: 78 00 00 00
command: 01 00 00 00
#
# Model: Yamaha ZP45780
#
name: Prev
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6A 95 00 00
#
name: Next
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 6B 94 00 00
#
name: Play
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 68 97 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 67 98 00 00
#
name: Pause
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 69 96 00 00
#
# Model : NAD DR2 remote for NAD D7050 and D3020
#
name: Power
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 25 DA 00 00
#
name: Vol_up
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 88 77 00 00
#
name: Vol_dn
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 8C 73 00 00
#
name: Mute
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 94 6B 00 00
#
name: Next
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 1A E5 00 00
#
name: Prev
type: parsed
protocol: NECext
address: 87 7C 00 00
command: 1D E2 00 00
#
# Model: JVC RM-SRVNB1A for JVC RV-NB1 boombox (2004)
#
name: Power
type: raw
frequency: 38000
duty_cycle: 0.333333
data: 8400 4200 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 25248 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 33664
#
name: Vol_up
type: raw
frequency: 38000
duty_cycle: 0.333333
data: 8400 4200 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 25248 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 526 526 33664
#
name: Vol_dn
type: raw
frequency: 38000
duty_cycle: 0.333333
data: 8400 4200 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 25248 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 1578 526 526 526 526 526 526 526 526 526 526 526 526 526 33664
#
name: Next
type: raw
frequency: 38000
duty_cycle: 0.333333
data: 8400 4200 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 1578 526 526 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 25248 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 1578 526 526 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 33664
#
name: Prev
type: raw
frequency: 38000
duty_cycle: 0.333333
data: 8400 4200 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 25248 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 1578 526 526 526 1578 526 1578 526 1578 526 1578 526 1578 526 526 526 526 526 33664
#
