Filetype: IR tests file
Version: 1
#
name: encoder_decoder_input1
type: parsed_array
count: 26
#
protocol: NEC42
address: 00 00 00 00
command: 00 00 00 00
repeat: false
#
protocol: NEC42
address: 01 00 00 00
command: 00 00 00 00
repeat: false
#
protocol: NEC42
address: 01 00 00 00
command: 80 00 00 00
repeat: false
#
protocol: NEC42
address: 00 00 00 00
command: 80 00 00 00
repeat: false
#
protocol: NEC42
address: 00 00 00 00
command: 00 00 00 00
repeat: false
#
protocol: NEC42
address: 00 00 00 00
command: 00 00 00 00
repeat: true
#
protocol: NEC42
address: 00 00 00 00
command: 00 00 00 00
repeat: false
#
protocol: NEC42
address: 00 00 00 00
command: 00 00 00 00
repeat: true
#
protocol: NEC42
address: FF 1F 00 00
command: FF 00 00 00
repeat: false
#
protocol: NEC42
address: FE 1F 00 00
command: FF 00 00 00
repeat: false
#
protocol: NEC42
address: FE 1F 00 00
command: 7F 00 00 00
repeat: false
#
protocol: NEC42
address: FF 1F 00 00
command: 7F 00 00 00
repeat: false
#
protocol: NEC42
address: FF 1F 00 00
command: FF 00 00 00
repeat: false
#
protocol: NEC42
address: FF 1F 00 00
command: FF 00 00 00
repeat: true
#
protocol: NEC42
address: AA 0A 00 00
command: 55 00 00 00
repeat: false
#
protocol: NEC42
address: 55 15 00 00
command: AA 00 00 00
repeat: false
#
protocol: NEC42
address: 55 15 00 00
command: 55 00 00 00
repeat: false
#
protocol: NEC42
address: AA 0A 00 00
command: AA 00 00 00
repeat: false
#
protocol: NEC42
address: AA 0A 00 00
command: AA 00 00 00
repeat: true
#
protocol: NEC42
address: AA 0A 00 00
command: AA 00 00 00
repeat: false
#
protocol: NEC42
address: AA 0A 00 00
command: AA 00 00 00
repeat: true
#
protocol: NEC42
address: AA 0A 00 00
command: AA 00 00 00
repeat: true
#
protocol: NEC42
address: 55 15 00 00
command: 55 00 00 00
repeat: false
#
protocol: NEC42
address: 55 15 00 00
command: 55 00 00 00
repeat: true
#
protocol: NEC42
address: 55 15 00 00
command: 55 00 00 00
repeat: true
#
protocol: NEC42
address: 55 15 00 00
command: 55 00 00 00
repeat: true
#
