// <<< Use Configuration Wizard in Context Menu >>>

// <h> Debug Setup

// <o> Release M0 On Connect
//   <0=> No
//   <1=> Yes
// <i> Debugger releases the M0 Application processor from reset when connecting to it.
ReleaseM0OnConnect = 1;

// <o> Release M0 Sub-System On Connect
//   <0=> No
//   <1=> Yes
// <i> Debugger releases the M0 Sub-System from reset when connecting to it (LPC437x only).
ReleaseM0SubOnConnect = 1;

// <o> Vector Reset
//   <0=> Processor Only
//   <1=> Processor and Peripherals
// <i> Select if to additionally reset peripherals (LCD, USB0, USB1, DMA, SDIO, ETHERNET) after a Vector Reset
VecResetWithPeriph = 1;

// </h>

// <h> TPIU Pin Routing (TRACECLK fixed on PF_4)
// <i> Configure the TPIU pin routing as used on your target platform.
// <o.1> TRACEDATA0
//   <0=> Pin PF_5
//   <1=> Pin P7_4
// <o.2> TRACEDATA1
//   <0=> Pin PF_6
//   <1=> Pin P7_5
// <o.3> TRACEDATA2
//   <0=> Pin PF_7
//   <1=> Pin P7_6
// <o.4> TRACEDATA3
//   <0=> Pin PF_8
//   <1=> Pin P7_7
RoutingTPIU = 0x00000000;

// </h>

// <<< end of configuration section >>>
